Version 7.0 (November 7, 2002)
--------------------------------------------------------------------------

This file contains information regarding the corrections, modifications 
and enhancements that have been made since the release of version 5.005.

Depending on the specific edition that you are using, different features
are available. Although all features are described in this Readme file,
they may not be available in your edition of the software.

--------------------------------------------------------------------------

Table of Contents:
1. New Features & Enhancements
2. Bugs and Fixes
3. Printer-specific Fixes and Corrections
4. New Printer Drivers
5. Instructions for Installing USB Hasp Key

--------------------------------------------------------------------------


1. New Features & Enhancements:
-------------------------------

- New "Shape" feature allows users to add a variety of shape types (Arrows,
  Packaging, Tools, etc.) to their labels. Users can also add their own custom
  company- or industry-specific graphics as shapes by creating a Windows Metafile
  and saving it in a subfolder within the program's Shapes folder.

- Added support for the new PLANET Code U.S. Postal Service bar code.

- New Pick List option added to Keyboard Input data origin. The Pick List allows
  users to select data from a pre-configured drop-down list at print time,
  ensuring error-free data entry.

- Double Entry Verification feature added to validate Keyboard Input data at
  print time by requiring the user to double enter the data.  The two entries
  are then compared to ensure they match. 

- New LogView feature allows the user to create custom reports from the log
  files created by using the Write Data function.

- The internal database module has been replaced with an updated database editor
  program that supports more database types. The database module now reads and
  writes dBase (dBaseIII or IV) files, and if ODBC drivers are installed on your
  PC, it can be used to modify these source files as well.

- Windows print spooling ability added, allowing thermal printers to use the
  Windows print spooler to manage print jobs using the queuing ability of the
  print spooler.



2. BUGS AND FIXES:
------------------

*******
General
*******

- Fixed problem causing a Win95 PC to crash, resulting in the .QDF files not opening.

- Program no longer generates virtual memory errors when trying to open a label. 

- UNC path for a graphic image will now display on the label and print correctly.

- If using a USB security key with the software, note that you must reboot the 
  computer after install in order for Windows to load the proper driver for the key.


**********
Duplicates
**********

- Fixed problem with Visual FoxPro memo fields only printing a paragraph on the
  first duplicate when the label has multiple labels per page.

- Fixed problem with Memo fields from Access only printing on the first duplicate.

- With  a duplicate count set to Keyboard input, the program no longer causes the
  label not to print until pressing Print Labels for the next label or pressing Quit.

- Fixed problem when printing using a primary key with a duplicate setup – if an
  incorrect record was selected and the BACK button was pressed, the first record
  (incorrect) would still print.


*********************
Keyed Database Access
*********************

- Fixed problem with an MS Access database in form layout. When entering a primary
  key at print time, user would receive error: "No matching key found."

- IP connection no longer gets broken when leaving the keyed access dialog open
  without sending a job.

- Fixed problem with using SQL Sever and SQL statements where at print time
  if you choose a specific record and check the Print All Matching Records box,
  you would receive an error message: "UCASE is not a recognized built in
  function name."

- Program no longer generates the database error: "Rows to update cannot be
  found" when selecting the same record (only one record), using Keyboard
  Input, and printing the labels.

- The primary key is now found with an AS400 ODBC driver connecting directly
  to the AS400 (not file).

- When printing from a FoxPro database, the program now prints just the sorted
  records instead of printing all matching records from the total database. 

- Fixed problem in versions 5.00.05 and .06 where keyed access screen would
  not display ANY of the records.


********
LMWPrint
********

- When using a password, LMWPrint.exe now closes down when job is done.

- New LMWPrint command for AutoPrint to create a backup of the database file.

- When using LMWPrint with AutoPrint, program now ensures that the database file
  can be successfully read before beginning to print.



3. Printer-specific Fixes and Corrections:
------------------------------------------

- Datamax E4203: Program will now cut at the end of a batch.

- Eltron TLP 2742: Fixed issues with MaxiCode "Zip Code" field for Puerto Rico.

- Intermec 4420 & 3400 C&D: Graphic images will now print correctly.

- Monarch 9850: When using a TrueType font the first field on the label will now
  print correctly on every other label printed.

- Printronix T5208: Program now scales the thermal printer's internal font properly. 

- Sato CT400: Fixed problem with the #Eab command being sent incorrectly; should
  be of the format #Eba instead.

- Sato 8400S: Fixed problem with upside down print direction no updating the time.

- Sato M-8400S: When printing labels with the duplicate count set at 9999, the
  program now correctly clears the print buffer after printing the labels.

- Zebra 105se: Program no longer sends down print speed per print job instead of
  per label.

- Zebra 220 Xi: Fixed problem where the Pause Count was ignored, cutting every
  label instead of every 6th label.

- Zebra T402: Fixed problem with printing off the label to the right.



4. NEW PRINTER DRIVERS:
-----------------------
The following printer drivers have been added in LABEL MATRIX 7.0:

Cognitive Del Sol 300 DPI
Datamax DMX E-4204
Dunbar APS
Eltron Orion LP2443
Facit D455
Facit D466
Facit D470/152
Facit D480 (300 dpi)
Facit D660
Fox IV 8000 (203 dpi)
Fox IV 8000 (300 dpi)
Fox IV 8031 Turbo (203 dpi)
Fox IV 8031 Turbo (300 dpi)
Fox IV 8031M (203 dpi)
Fox IV 8031M (300 dpi)
Fox IV 8031S (203 dpi)
Fox IV 8031S (300 dpi)
Fox IV 8041 Turbo (203 dpi)
Fox IV 8041 Turbo (300 dpi)
Fox IV 8041M (203 dpi)
Fox IV 8041M (300 dpi)
Fox IV 8041S (203 dpi)
Fox IV 8041S (300 dpi)
Fox IV 8200
Fox IV 8231 Turbo
Fox IV 8231M
Fox IV 8231S
Fox IV 8600
Fox IV 8641
Imaje ITP/400
Imaje ITP/430
Imaje ITP/600
Imaje ITP/800
Imaje ITP/Datolabel
Imaje ITP/Datolabel Plus
Imaje ITP/La Mini
Impuls One-DT D
Legi 700-3210
Legi 700-4206
Legi 700-4212
Legi 700-4308
Legi 700-6208
Legi 700-6308
Legi 700-8306
Legi 770
Legi 770-2
Legi 771
Legi 772
Legi 773
Legi 774
Legi 774-2
Legi 775
Legi 776 (152 dpi)
Legi 776 (203 dpi)
Legi 776+ (203 dpi)
Legi 776+ (300 dpi)
Legi 777
Legi 794
Markpoint MP104 Compact RFID 203 DPI
Markpoint MP104 Compact RFID 300 DPI
Meto LS 40
Meto mi-4208
Monarch 9414M
Monarch 9825 (203 DPI)
MPH Delta 344 DL
MPH Golf 244 DL
MPH Golf 248 DL
MPH Golf 344 DL5
Sato CX208DT
Sato CX208TT
Sato CX212DT
Sato CX212TT
TEC B-452-HS
TEC B-852
Zebra Orion LP2443



5. Instructions for Installing USB Hasp Key:
--------------------------------------------

1. Begin installation.

2. At the screen for security key check, press the INSTALL DRIVER button.

3. Plug in the Key -- win98 should detect the key and launch the new hardware wizard. 
Advance through the wizard searching for a driver. Click the FINISH button when no
driver is found.

4. Continue installation for LABEL MATRIX (MDAC may need to be installed also 
and force a reboot before installation is complete). DO NOT RESTART yet.

5. Go to Windows Device Manager. Select unknown devices tab. HASP4 USB 
should be there. Remove the device from system.

6. Restart the PC.

7. Upon reboot, the PC should automaticallly recognize hardware and find driver.

8. If Win98 does not 'see' the driver, point to the following dir path: 

   C:\WINDOWS\SYSTEM

9. Win98 should now see the driver.
